e2e_plot_edrivers {StrathE2E2} | R Documentation

## Plot climatological year of environmental driving data.

### Description

Multi-panel time series plots of climatological annual cycles of driving data as provided in the input csv files.

### Usage

    e2e_plot_edrivers(model)

### Arguments

`model` | R-list object defining the model configuration compiled by the e2e_read() function.

### Details

The function plots a multi-panel page of time series plots of monthly values of the environmental driving data for the model.

Units for the plotted variables are as follows:

- Sea surface irradiance: uE/m2/d

- Suspended particulate matter: g/m3

- Temperature: deg-C

- Vertical diffusivity gradient: m/d (derived from the vertical diffusivity (m2/s) and mixing length scale (m))

- External inflows: m3 per m2 sea surface of model domain (derived from proportion input per layer volume, layer thicknesses and areas)

- River discharge: m3 per m2 sea surface of model domain (derived from proportion input to inshore volume, and inshore layer thickness and area)

- Inshore significant wave height: m

- Proportion of seabed disturbed: /d (aggregated over the three sediment classes in each zone)

- External boundary nitrate concentration: mMN/m3

- External boundary ammonia concentration: mMN/m3

- External boundary phytoplankton concentration: mMN/m3

- External boundary detritus concentration: mMN/m3

- River nitrate concentration: mMN/m3

- River ammonia concentration: mMN/m3

- Atmospheric nitrate deposition flux: mMN/m2/d

- Atmospheric ammonia deposition flux: mMN/m2/d

### Value

Graphical display in a new graphics window. Does not return any data object since the data plotted are all available as input csv files.

### See Also

`e2e_read`, `e2e_run`, `e2e_plot_fdrivers`

### Examples

    # Load the 2003-2013 version of the North Sea model supplied with the package:
        model <- e2e_read("North_Sea", "2003-2013")
    # Plot the annual cyles of driving data
        e2e_plot_edrivers(model)

    # Direct the graphics output to a pdf file ...
    # or jpeg("plot.jpg"), png("plot.png")
        pdf(file.path(tempdir(), "plot.pdf"),width=8,height=6)
        e2e_plot_edrivers(model)
        dev.off()

[Package StrathE2E2 version 3.2.0 Index]